Based on the development of Frictionless Surfaces, the Stealth Sub uses a material similar to sharkskin to part the water and glide at near zero friction and noise. This allows the Sub to concentrate on active and passive sonar avoidance: using thermal layers to deflect sonar pulses and using a magneto-hydro-dynamic pulsar engine to slip past listening microphones.